Geologic map of the Sperry 7.5¢ quadrangle, Tulsa County, Oklahoma

Frequently asked questions:
•	What does the data describe? 
•	How should the data be cited? 
•	What geographic area does the data cover?
•	What does it look like?
•	Does the data describe conditions during a particular time period? 
•	How are geographic features stored in the data? 
•	What coordinate system is used to represent geographic features? 
•	How does the data describe geographic features? 
•	Who are the originators of the data? 
•	Who also contributed to the data? 
•	To whom should users address questions about the data? 
•	Why was the data created? 
•	From what previous works were the data drawn? 
•	How were the data generated, processed, and modified? 
•	How reliable are the data; what problems remain in the data? 
•	Are there legal restrictions on access or use of the data? 
•	Who distributes the data? 
•	What's the catalog number I need to order the data? 
•	What legal disclaimers am I supposed to read? 
•	How can I download or order the data? 
•	Who wrote the metadata? 

What does the data describe?
Title:  Geologic map of the Sperry 7.5¢ quadrangle, Tulsa County, Oklahoma.

Abstract:  The geologic map of the Sperry quadrangle was compiled from detailed field mapping and field investigations by the authors.  The geology was manually constructed onto a modern 7.5¢ topographic quadrangle for ultimate publication at a scale of 1:24,000.

How should the data be cited? 

Miller, Galen W.; and Stanley, Thomas M., 2005, Geologic map of the Sperry 7.5¢ quadrangle, Tulsa County, Oklahoma: Oklahoma Geological Survey Oklahoma Geologic Quadrangle OGQ-61, scale 1:24,000.
What geographic area does the data cover?
West Bounding Coordinate:  -96.00
East Bounding Coordinate:  -95.875
North Bounding Coordinate:  36.375
South Bounding Coordinate:  36.25
What does it look like?
A PDF of the published geologic map, a zipped (ZIP) file containing all the geologic map features in an ESRI shapefile format, and a metadata document
Does the data describe conditions during a particular time period?
Calendar Date:  2005
Currentness Reference:  Publication date 
How are geographic features stored in the data?
PDF and ESRI shapefile format
What coordinate system is used to represent geographic features?
Grid Coordinate System:  Universal Transverse Mercator
UTM Zone: 15N
Scale Factor at Central Meridian:  0.99960
Longitude of Central Meridian:  -93.00
Latitude of Projection Origin:  0.00
False Easting:  500000.00
False Northing:  0.00
Planar Coordinates:  Meters
Horizontal Datum:  North American Datum 1927 (NAD27)
Ellipsoid:  Clarke 1866
Semi-Major Axis of the Ellipsoid:  6378206.40
Flattening of the Ellipsoid:  1/294.9786980
How does the data describe geographic features?
The published geologic map of the Sperry 7.5¢ quadrangle uses a digital U.S. Geological Survey 1:24,000 topographic base map, where symbols and line work are the same as those found on the published U.S. Geological Survey 1:24,000 paper topographic map for the quadrangle. Geologic symbols and line work are shown in the explanation on the map. Structural information and how the areal extent of geologic units is shown, also are typical of geologic maps published by the USGS and other state geological surveys. The PDF file is a digital representation of a paper geologic map and all the topographic and geologic symbols are the same as those used on commonly used and widely accessible federal- and state-survey-produced geologic maps. The geologic symbols conform closely, but not exact in every case, to the FGDC Digital Cartographic Standard for Geologic Map Symbolization. The ESRI shapefiles of the geologic map can be symbolized by the user to represent the published map or other geologic standards.
Who are the originators of the data?
Geologists:  Galen W. Miller and Thomas M. Stanley
Digital Cartographer:  G. Russell Standridge
Who also contributed to the data?
Manager of OGS Cartographic Section:  James H. Anderson
To whom should users address questions about the data?
Thomas M. Stanley
Oklahoma Geological Survey
100 E. Boyd St., Rm. N-131
Norman, Oklahoma  73019
Phone:  (405) 325-3031
Fax:  (405) 325-7069
E-mail:   tmstanley@ou.edu
Why was the data created?
The data was created to provide a geologic map of the Sperry 7.5¢ quadrangle. The map or any parts of it can be printed or viewed at a variety of scales and be used in many ways by homeowners, landowners, civil engineers, land-use planners, government agencies, businesses, etc. This map data is not meant to be used or displayed at any scale larger than 1:24,000 (e.g., 1:20,000 or 1:12,000).
From what previous works were the data drawn?
Bennison, A.P.; Chenoweth, P.A.; Desjardins, J.; and Ferris, C., 1972, Surface geology and Bouguer gravity of Tulsa County, Oklahoma. In, A.P. Bennison (ed.), Tulsa’s Physical Environment: Tulsa Geological Society Digest, 37, 352 p.
Marcher, M.V.; and Bingham, R.H., 1971, Reconnaissance of the water resources of the Tulsa quadrangle, northeastern Oklahoma: Oklahoma Geological Survey Hydrologic Atlas Map HA-2, sheet 1 (of 4), scale 1:250,000. 
Oakes, M.C., 1952, Geology and mineral resources of Tulsa County, Oklahoma (includes parts of adjacent counties): Oklahoma Geological Survey Bulletin, 69, 234 p.
How were the data generated, processed, and modified?
Previously published reports (see above) were consulted in order to establish the stratigraphic framework and general geologic relations of the area. These reports, however, served only as a general guide. A 7.5¢ topographic map of the area was taken into the field and used as the base map for compiling the geology of the quadrangle. Because much of the area is urban, virtually all the roads in the area were driven and any outcrops were checked and described; these outcrops are noted on the map. In some cases walking traverses were made to look for additional outcrops. The cross section is based on the surface geology (this map), in conjunction with any subsurface data, such as lithologies and lithologic contacts, that could be derived from drill hole wire-line logs and drill cutting logs stored at the Oklahoma Geological Survey’s OPIC facilities.  

The geology and cross section were digitized at a scale of 1:24,000 with wells, geologic observations, individual map units, or other mappable features as separate layers in an ESRI shapefile format. All shapefiles are then assembled together and overlain by a USGS 1:24,000-scale topographic base map. Symbology and labels were designated for a final map layout at 1:24,000 scale. The final map was then published Oklahoma Geologic Quadrangle OGQ-61 as a PDF along with the data files in ESRI shapefile format.

How reliable are the data; what problems remain in the data?
The geologic map is based on detailed field mapping and interpretation of additional data by the authors at a 1:24,000 scale. Most of the contacts bordering Quaternary units are gradational. The locations of the petroleum wells are based on data available in the Natural Resources Information System (NRIS) database; these records, in turn, are based on forms submitted by individual operators to the Oklahoma Corporation Commission. The locations of petroleum wells were not verified in the field.  The records maintained in the NRIS database may be incorrect and/or incomplete; thus, the well locations shown on the map may be incomplete and/or incorrect.
The format of the data as an ESRI shapefile was originally used as a cartographic tool for constructing a printable map. The map was digitized at a scale of 1:24,000. Errors may exist from the digitizing process done at that scale. This may include errors in relation to the locational accuracy and precision of:  the contact or map unit boundary to the topographic contour; a map unit layer to another map unit layer (e.g., gaps, overlaps, slivers, overshoots). These data and adjoining data for other quadrangles were produced on a quadrangle-by-quadrangle basis. Therefore, misalignment issues may exist between these data and other data downloaded for adjoining quadrangles. Also, the attribute table for each geologic feature layer may not contain detailed information except when used for categorizing some feature objects. Specific information about each geologic unit can be found in the Description of Units on the published PDF map. Currently underway, these issues are being resolved for each quadrangle map through revision and implementation of a geologic data model based on an ESRI geodatabase environment. These revised data files will be available for download on the OGS website in the near future.

Are there legal restrictions on access or use of the data?

Access Constraints:  None

Use Constraints:  This digital map is not meant to be used or displayed at any scale greater than 1:24,000. Users should cite the Oklahoma Geological Survey as the original source of the data, but clearly denote cases where the original data has been updated, modified, or in any way altered from the original condition. There are no restrictions on the distribution of the data or interpretations shown on this data or reproduction of the data from the graphics files. However, users are encouraged to refer others to the Oklahoma Geological Survey to acquire the original data or any updated versions of the data.
Who distributes the data?
Oklahoma Geological Survey
100 E. Boyd St., Rm. N-131
Norman, OK  73019
What's the catalog number I need to download the data?
Oklahoma Geologic Quadrangle OGQ-61.
What legal disclaimers am I supposed to read?
The Oklahoma Geological Survey (OGS) provides these geologic data “as is”. The OGS makes no guarantee or warranty concerning the accuracy of information contained in the data. The OGS further makes no warranties, either expressed or implied, as to any other matter whatsoever including, without limitation, the condition of the product, or its fitness for any particular purpose. The burden for determining fitness for use lies entirely with the user. Although these data have been processed successfully on computers at the OGS, no warranty, expressed or implied, is made by the OGS regarding the use of these data on any other system, nor does the fact of distribution constitute or imply any such warranty.
In no event shall the OGS have any liability whatsoever for payment of any consequential, incidental, indirect, special, or tort damages of any kind, including, but not limited to, any loss of profits arising out of use of or reliance on the geologic data or arising out of the delivery, installation, operation, or support by OGS.
This digital geologic map of the Sperry 7.5¢ quadrangle, Tulsa County, Oklahoma is not meant to be used or displayed at any scale larger than 1:24,000.
How can I download or order the data?
Availability in Digital Form:
Data Format:
PDF and ESRI shapefile		
Free Download at:  
Oklahoma Geological Survey website
http://www.ogs.ou.edu/geolmapping.php
Who wrote the metadata?
	Dates: 
Last Modified:  February 2007

Metadata Author:
Oklahoma Geological Survey
c/o Thomas M. Stanley and/or G. Russell Standridge
100 E. Boyd St., Rm. N-131
Norman, OK  73019
Phone (405) 325-3031
Fax (405) 325-7069